{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["工程量清单","兴企路西侧建筑物","兴企路西侧构筑物、附属物"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量清单","index":0,"n_rows":6,"n_cols":1,"rows_kept":6,"flags":["formulas_cached_only"]}
[]
["河南中原黄金冶炼厂有限责任公司退役厂区建筑物、构筑物拆除工程二标段（兴企路西侧）工程"]
[]
[]
[]
["招 标 工 程 量 清 单"]

{"sheet":"兴企路西侧建筑物","index":1,"n_rows":105,"n_cols":6,"rows_kept":105,"merged":[[0,0,0,5],[103,0,103,1],[104,0,104,5]],"flags":["formulas_cached_only"]}
["兴企路西侧建筑物拆除明细表"]
["航拍编号","资产名称/用途","建筑面积（㎡）","单价","合价","备注"]
[42,"高配站",583.44,null,null,"1层混合结构"]
[43,"冶炼分厂办公楼",{"v":606.5,"d":"606.50"},null,null,"2层混合结构"]
[44,"冶炼厂维修",353.35,null,null,"2层混合结构"]
[45,"净化泵房",{"v":106.4,"d":"106.40"},null,null,"高7.35m，焙1净化系统框架一层"]
[46,"净化泵房配电室",{"v":17.9,"d":"17.90"},null,null,"焙1净化系统框架一层"]
[47,"净化工段",149.55,null,null,"1层混合结构"]
[48,"焙Ⅰ制酸工段办公楼及化验室",774.75,null,null,"2层混合结构"]
[49,"循环水泵站",537.14,null,null,"384.03㎡高度8.7m、下沉3.35m；剩余面积高度4.25m"]
[50,"铁红仓库",2890.87,null,null,"高度7.2m"]
[51,"干燥烘干机彩钢房",54.54,null,null,"1层彩钢结构"]
[52,"阳极保护泵房",48.71,null,null,"2层混合结构"]
[53,"制酸分厂干吸车间",238.16,null,null,"高度10.9m"]
[54,"硫酸储藏间",179.04,null,null,"高度10.3m"]
[55,"焙Ⅱ配电室 ",104.14,null,null,"1层混合结构"]
[56,"焙Ⅱ二氧化硫风机房",171.35,null,null,"复合板房"]
[57,"干吸",{"v":121.5,"d":"121.50"},null,null,"高6.85"]
[58,"二氧化硫风机房",611.33,null,null,"一层层高7.75m、二层层高4.4m、8.5m"]
[59,"制酸分厂配电室",185.35,null,null,"1层混合结构"]
[60,"焙Ⅱ配电室1",32.13,null,null,"1层混合结构"]
[61,"焙Ⅱ配电室2",158.53,null,null,"1层混合结构"]
[62,"酸浸操作室1",721.98,null,null,"高度7.7m、8.0m"]
[63,"酸浸操作室2",365.94,null,null,"高度4.0m、5.7m、4.1m"]
[64,"冶炼分厂维修工段",143.69,null,null,"高度5.1m"]
[65,"高温排风机房",276.34,null,null,"一层层高9m、二层层高3.5m、5.5m"]
[66,"电收尘操作室",20.48,null,null,"1层混合结构"]
[67,"焙烧Ⅰ配电室1",34.96,null,null,"高度6.6m"]
[68,"焙烧Ⅰ配电室2",99.56,null,null,"高度4.4m"]
[69,"罗茨风机房1",{"v":365.5,"d":"365.50"},null,null,"高度7.5m"]
[70,"焙烧Ⅰ工段值班室",68.75,null,null,"高度3.2m、6.2m"]
[71,"调浆间",{"v":245.7,"d":"245.70"},null,null,"高度18.6m"]
[72,"传送带通道3",{"v":169.8,"d":"169.80"}]
[73,"金矿仓储藏间",{"v":14.1,"d":"14.10"},null,null,"1层混合结构"]
[74,"泵房",53.51,null,null,"1层混合结构"]
[75,"淋浴房",373.87]
[79,"动力分厂办公室及电修车间",{"v":935.6,"d":"935.60"},null,null,"一层308.10㎡高度8.3m其余为两层"]
[80,"动力分厂电修车间1",{"v":344.8,"d":"344.80"},null,null,"265.94㎡高度4.3m剩余面积高度8.7m"]
[87,"原料库东门卫",52.01]
[88,"精矿仓库（原料仓）",1972.53,null,null,"高度16.8m、内有3.4m深的基坑"]
[89,"金矿仓更衣室",361.92]
[90,"配电室",104.39,null,null,"1层混合结构"]
[91,"焙Ⅱ净化更衣室",131.75,null,null,"1层混合结构"]
[92,"厕所1",33.97]
[93,"罗茨风机房2",{"v":118.5,"d":"118.50"},null,null,"简易房"]
[94,"焙Ⅱ浓密机操作间",17.33,null,null,"1层混合结构"]
[95,"冲渣泵房",{"v":31,"d":"31.00"},null,null,"证载"]
[96,"水井房3",{"v":28,"d":"28.00"},null,null,"1层混合结构"]
[97,"油库",76.88,null,null,"1层混合结构"]
[98,"加压循环水泵房",208.63]
[99,"西门门卫室",65.28]
[100,"老备件库",479.75,null,null,"高度4.3m"]
[101,"地磅房1",217.77]
[102,"地磅房2",132.09]
[103,"原料库西门门卫室",31.05]
[104,"传送带通道4",{"v":133,"d":"133.00"}]
[105,"锅炉房进料间1",{"v":219.1,"d":"219.10"},null,null,"1层混合结构"]
[106,"锅炉房进料间2",{"v":862.4,"d":"862.40"},null,null,"1层混合结构"]
[107,"锅炉房净化水1",371.85,null,null,"钢板顶、高度7m"]
[108,"锅炉房净化水2",74.88,null,null,"高度7m"]
[109,"锅炉房值班室",593.28,null,null,"3层混合结构"]
[110,"焙Ⅱ锅炉房",{"v":784,"d":"784.00"},null,null,"高度20.3m"]
[111,"传送带通道5",{"v":132,"d":"132.00"}]
[112,"锅炉工段储藏间",{"v":72.9,"d":"72.90"},null,null,"1层混合结构"]
[113,"水井房4",21.28,null,null,"1层混合结构"]
[114,"水井房5",10.24,null,null,"1层混合结构"]
[115,"铁路线值班室1",101.49,null,null,"1层混合结构"]
[116,"警卫室",{"v":27.6,"d":"27.60"}]
[117,"厕所2",{"v":8,"d":"8.00"}]
[118,"老酸段值班室",85.27,null,null,"1层混合结构"]
[119,"酸库值班室1",94.53,null,null,"高度4m"]
[120,"酸库值班室2",180.03,null,null,"高度7.3m、下沉2.4m"]
[121,"酸库小仓库",80.63]
[122,"铁路线值班室2",19.66,null,null,"1层混合结构"]
[123,"水井房6",{"v":22.7,"d":"22.70"}]
[124,"水井房7",8.79,null,null,"1层混合结构"]
[125,"造纸厂车间1 ",245.99,null,null,"1层混合结构"]
[126,"造纸厂车间2",245.99,null,null,"1层混合结构"]
[127,"造纸厂车间3",{"v":123.2,"d":"123.20"},null,null,"1层混合结构"]
[128,"水井房8",24.69,null,null,"1层混合结构"]
[129,"西南门纸厂警卫室",28.51,null,null,"1层混合结构"]
[130,"水井房9",{"v":33,"d":"33.00"},null,null,"1层混合结构"]
[131,"杂物房",56.35,null,null,"简易房"]
[132,"供应处办公室",163.42,null,null,"1层混合结构"]
[133,"仓库房",{"v":97.2,"d":"97.20"},null,null,"1层混合结构"]
[134,"纸厂办公楼",1613.36,null,null,"1层混合结构"]
[135,"纸厂值班室1",9.46,null,null,"1层混合结构"]
[136,"纸厂值班室2",{"v":40.5,"d":"40.50"},null,null,"简易房"]
[137,"供应处仓库门卫",{"v":24,"d":"24.00"},null,null,"复合板房"]
[138,"供应库",2305.47,null,null,"高度6.2m"]
[139,"供应处警卫室",{"v":24.2,"d":"24.20"},null,null,"复合板房"]
[140,"设备库",562.12,null,null,"1层混合结构"]
["棚 (15)","球磨机棚",{"v":414,"d":"414.00"},null,null,"拱高7.2m"]
["棚 (16)","循环水冷却塔设备搭棚",104.31]
["棚 (17)","焙Ⅱ车棚",109.15]
["棚 (18)","煤仓",1607.03,null,null,"顶高14.4m、内有3m深基坑及水池"]
["棚 (19)","矿粉堆砌棚",23.65]
["棚 (20)","洗袋区",321.75]
["棚 (21)","地磅房棚",203.37]
["棚 (22)","小仓库",13.38]
["棚 (23)","警卫室",10.02]
["棚 (24)","酸库值班室3",31.36]
[null,"铁红仓库值班室",{"v":5.5,"d":"5.50"}]
["合计"]
["建筑物拆除要求：地上建筑物全部拆除，地下的独立基础和桩承台全部拆除，装车和外运"]

{"sheet":"兴企路西侧构筑物、附属物","index":2,"n_rows":154,"n_cols":8,"rows_kept":154,"merged":[[0,1,0,7],[5,1,5,4],[43,1,43,4],[48,1,48,4],[57,1,57,4],[88,1,88,4],[94,1,94,4],[105,1,105,4],[153,0,153,2]],"flags":["formulas_cached_only"]}
[null,"兴企路西侧构筑物拆除明细表"]
["序号","类别","规格","单位","数量","单价","合价","备注"]
[1,"烟囱（塔1）","底部5.5m、顶部3m、高度60m","座",1]
[2,"烟囱（塔2）","底部9m、顶部6m、高度80m","座",1]
[3,"水塔（塔3）","底部5.5m、顶部4m、高度25m","座",1]
[4,"焙1基础区域："]
[5,"水泥地坪",null,"㎡",136.62,null,null,"地坪贴3层0.4玻璃丝布防腐处理，防腐瓷板"]
[6,"焙1酸浸M15浓密机","φ17m，地上2.2m，地下4.5m","个",1,null,null,"浓密机内表面贴10层0.4玻璃丝布防腐处理，防腐标砖"]
[7,"焙1电收尘框架","高8m","㎡",270.7]
[8,"焙1铁红浆液槽框架","高9.3m，2层","㎡",86.58,null,null,"其他面积已在建筑物明细表列明-酸浸操作室2"]
[9,"焙1铁红浆液槽基础","φ4.0m，地下1.5m，地上0.1m","个",7,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[10,"焙1铁红浆液槽基础","φ4.5m，地下1.5m，地上0.1m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[11,"焙1铁红浆液槽基础","φ2.7m，地下1.5m，地上0.1m","个",3,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[12,"焙1滤液槽基础","φ4.5m，地下1.5m，地上0.1m","个",2,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[13,"焙1滤液槽基础","φ2.7m，地下1.5m，地上0.1m","个",3,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[14,"焙1滤液槽基础","φ4.0m，地下1.5m，地上0.1m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[15,"焙1焙烧炉框架","高8m","㎡",239.25]
[16,"焙1旋风收尘框架","高16.2m，3层","㎡",351.75]
[17,"焙1胶带机框架","高6.4m","㎡",227.13,null,null,"混凝土平台上面贴3层0.4玻璃丝布防腐处理，防腐瓷板"]
[18,"焙1胶带机框架地下水池","深5.5m","㎡",101.2,null,null,"内表面外贴6层0.4玻璃丝布防腐处理"]
[19,"槽基础","φ4.5m，地下1.5m，地上0.7m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[20,"槽基础","φ2.6m，地下1.5m，地上0.7m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[21,"槽基础","φ3.3m，地下1.5m，地上0.7m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[22,"钢架棚",null,"㎡",227.13]
[23,"焙1沉淀池","深3.2m","㎡",44.16]
[24,"焙1沉淀池","深1.2m","㎡",44.16]
[25,"焙1滤液池","深4.0m","㎡",50.8,null,null,"内表面外贴6层0.4玻璃丝布防腐处理"]
[26,"硬化",null,"㎡",728.53,null,null,"地坪贴3层0.4玻璃丝布防腐处理，防腐瓷板"]
[27,"焙1硫酸储罐基础","φ10.7m，地下1.5m","个",1]
[28,"硫酸储罐周围地坪",null,"㎡",164.53,null,null,"地坪贴3层0.4玻璃丝布防腐处理，防腐瓷板"]
[29,"焙1装酸平台",null,"㎡",59.92,null,null,"平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[30,"硬化",null,"㎡",1634.92]
[31,"焙1转化器基础","φ6.6m，地下1.5m","个",2]
[32,"焙1转化器基础","φ3.4m，地下1.5m","个",6]
[33,"焙1转化器框架","高6.3m","㎡",46.92]
[34,"硬化",null,"㎡",965.91]
[35,"焙1干燥塔框架","高6.0m","㎡",19.63,null,null,"平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[36,"焙1冷却塔池","深2.0m","㎡",43.56]
[37,"冷却塔周围地坪",null,"㎡",391.45,null,null,"地坪表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[38,"焙1沉降槽基础框架","高5.3m","㎡",63.59]
[39,"焙1净化系统框架","高13.3m，2层","㎡",95,null,null,"每层平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[40,"焙1净化系统框架","高17m，2层","㎡",221.55,null,null,"每层平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[41,"焙1净化系统框架","高7.3m","㎡",108.75,null,null,"每层平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[42,"循环水、铁红冷却基础区域："]
[43,"铁红冷却塔池","深4.0m","㎡",222.6]
[44,"循环水冷却塔池","地下2.0m，地上10.5m","㎡",158.42]
[45,"循环水泵水池","深4.0m","㎡",58.14]
[46,"消防水池","深5.0m","㎡",140.4]
[47,"澡堂、球磨机基础区域："]
[48,"澡堂污水沉淀池","深1.5m","㎡",5.16]
[49,"原料皮带廊北冷却塔池","深1.5m","㎡",14.28]
[50,"棚15下基础（球磨基础）","深1.2m","㎡",6.48]
[51,"板框基础","长1.5m，宽0.6m，高0.5m","个",4]
[52,"球磨机储罐基础","φ3.6m，地下1.5m","个",1]
[53,"皮带廊池","深2.3m","㎡",41.52]
[54,"防尘网挡墙",null,"㎡",106.8]
[55,"50围墙","高1.0m","㎡",119.6]
[56,"焙2基础区域："]
[57,"M15浓密机池","φ15m，地上4.6m，地下3.0m","个",2,null,null,"浓密机内表面贴10层0.4玻璃丝布防腐处理，防腐标砖"]
[58,"焙2电收尘框架","高8.0m","㎡",216.6]
[59,"焙2电收尘框架下基础","长2m，宽2m，高0.2m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理"]
[60,"焙2酸浸搅拌槽基础","φ3.0m，地上1.1m，地下1.5m","个",3,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理"]
[61,"焙2酸浸搅拌槽基础","φ2.6m，地下1.5m","个",3,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理"]
[62,"焙2酸浸搅拌槽基础","φ4.1m，地上0.6m，地下1.5m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理"]
[63,"焙2酸浸搅拌槽基础","地上0.6m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理"]
[64,"焙2酸浸搅拌槽地坑","深4.5m","㎡",71.78,null,null,"基础外表面贴10层0.4玻璃丝布防腐处理"]
[65,"泵基础","高0.2m","个",1]
[66,"焙2余热铁炉框架","高5.2m","㎡",142.2]
[67,"焙2焙烧炉1","高5.6m","㎡",184.5]
[68,"焙2焙烧炉2","高4.6m","㎡",106.08]
[69,"炉前调浆槽基础","φ3.2m，地上0.2m，地下1.5m，","个",2]
[70,"焙2净化系统框架","高11.5m，3层","㎡",520.8,null,null,"每层平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[71,"焙2净化系统框架","高17.7m，5层","㎡",680,null,null,"第1层按房屋；每层平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[72,"焙2沉降槽框架","高3.2m","㎡",62.7,null,null,"平台上表面3层0.4玻璃丝布防腐处理，防腐瓷板"]
[73,"焙2净化储罐基础（焙2转化换热器基础）","φ3.0m，地下1.5m","个",4,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[74,"焙2净化储罐基础（焙2转化换热器基础）","φ4.5m，地下1.5m","个",2,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[75,"基础","高0.2m","个",1]
[76,"焙2冷却塔池1","高2.3m","㎡",59.29]
[77,"焙2冷却塔池2","高2.3m","㎡",44.89]
[78,"焙2冷却塔池2","高2.3m","㎡",57.76]
[79,"泵基础","高0.2m","个",1]
[80,"冷却塔北侧地坪",null,"㎡",254.82]
[81,"焙2干吸阳极保护基础","高0.8m","个",1,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[82,"硫酸储罐基础","φ3.4m，地下1.5m","个",2,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[83,"硫酸储罐基础","φ4.7m，地下1.5m","个",3,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[84,"焙2干洗塔基础框架","高5.5,3个","㎡",47.69]
[85,"焙2转化器基础","φ6.6m，地下1.5m，地上0.7m","个",1]
[86,"焙2干洗周围地坪",null,"㎡",615,null,null,"地坪贴6层0.4玻璃丝布防腐处理，防腐瓷板"]
[87,"煤渣池、锅炉房基础区域："]
[88,"煤渣池","深5.5m","㎡",127.6]
[89,"煤渣池","深3.0m","㎡",50]
[90,"锅炉房风机房",null,"㎡",54.32]
[91,"麻石除尘器","φ3.0m，石砌，厚30cm","㎡",13]
[92,"锅炉房电收尘框架","高7.5m","㎡",181.39]
[93,"原料仓区域："]
[94,"煤仓水泥柱","长1.2m，宽0.7m，高7m","个",40]
[95,"37围墙",null,"㎡",35.2]
[96,"50围墙",null,"㎡",885.2]
[97,"原料仓雨水池","深2.0m","㎡",153.99]
[98,"24围墙",null,"㎡",65]
[99,"24围墙",null,"㎡",144.45]
[100,"铁栅栏围墙","铁栅栏1.7m，砖墙0.7m","㎡",147.6]
[101,"电动伸缩门",null,"m",15.6]
[102,"生活污水处理箱",null,"㎡",42]
[103,"50围墙",null,"㎡",301.76]
[104,"西料场区域："]
[105,"行吊车基础","深1.5m，2道","道",2]
[106,"西料场雨水沉淀池","深2.0m","㎡",47.84]
[107,"雨水池",null,"㎡",576]
[108,"钢架基础-JD-1","厚度1.5m，面积171.7㎡","个",1]
[109,"钢架基础-JD-2","厚度1.5m，面积35.22㎡","个",1]
[110,"钢架基础-JD-3","厚度1.5m，面25.61㎡","个",1]
[111,"钢架基础-JD-4","厚度1.5m，面积31.87㎡","个",1]
[112,"钢架基础-JD-5","厚度1.5m，面积17.71㎡","个",1]
[113,"钢架基础-JD-6","厚度1.5m，面积4.66㎡","个",1]
[114,"钢架基础-JD-7","厚度1.5m，面积9.42㎡","个",1]
[115,"钢架基础-JD-8","厚度1.5m，面积3.32㎡","个",1]
[116,"钢架基础-JD-9","厚度1.5m，面积4.71㎡","个",1]
[117,"钢架基础-JD-10","厚度1.5m，面积3.92㎡","个",1]
[118,"钢架基础-JD-11","厚度1.5m，面积7.56㎡","个",1]
[119,"钢架基础-JD-12","厚度1.5m，面积467.46㎡","个",1]
[120,"钢架基础-JD-13","厚度1.5m，面积37.1㎡","个",1]
[121,"钢架基础-JD-14","厚度1.5m，面积22.05㎡","个",1]
[122,"钢架基础-JD-15","厚度1.5m，面积114.48㎡","个",1]
[123,"钢架基础-JD-16","厚度1.5m，面积38.16㎡","个",1]
[124,"钢架基础-JD-17","厚度1.5m，面积47.25㎡","个",1]
[125,"钢架基础-JD-18","厚度1.5m，面积269.28㎡","个",1]
[126,"钢架基础-JD-19","厚度1.5m，面积67.5㎡","个",1]
[127,"钢架基础-JD-20","厚度1.5m，面积346.5㎡","个",1]
[128,"钢架基础-JD-21","厚度1.5m，面积4.86㎡","个",1]
[129,"钢架基础-JD-22","厚度1.5m，面积9.38㎡","个",1]
[130,"钢架基础-JD-23","厚度1.5m，面积18.75㎡","个",1]
[131,"水泥电线杆","高10m，带线","根",39]
[132,"排水沟","高0.8m","㎡",1765.4]
[133,"水井","H=120m","眼",8]
[134,"水泥地坪6",null,"㎡",5667]
[135,"水泥地坪7",null,"㎡",6210]
[136,"水泥地坪9",null,"㎡",9420]
[137,"水泥地坪10",null,"㎡",635]
[138,"水泥地坪11",null,"㎡",2111]
[139,"水泥地坪17",null,"㎡",967.5]
[140,"水泥地坪18",null,"㎡",162]
[141,"水泥地坪20",null,"㎡",704.34]
[142,"水泥地坪21",null,"㎡",1820.32]
[143,"水泥地坪22",null,"㎡",256]
[144,"水泥地坪24",null,"㎡",398.08]
[145,"水泥地坪25",null,"㎡",1302.5]
[146,"水泥地坪26",null,"㎡",155.49]
[147,"水泥地坪27",null,"㎡",7713.97]
[148,"水泥路面，园区道路","含路边排水沟和基础","㎡",1638.68]
[149,"水泥地坪6支架基础","厚度1.5m，46㎡","个",1]
[150,"水泥地坪6支架基础","厚度1.5m，24㎡","个",1]
[151,"硫酸储罐基础","φ13.0m，地上2米，地下2m","个",3]
["合计"]