{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["工程量清单","建筑物","构筑物、附属物"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"工程量清单","index":0,"n_rows":6,"n_cols":1,"rows_kept":6,"flags":["formulas_cached_only"]}
[]
["河南中原黄金冶炼厂有限责任公司退役厂区建筑物、构筑物拆除工程一标段（兴企路东侧）工程"]
[]
[]
[]
["招 标 工 程 量 清 单"]

{"sheet":"建筑物","index":1,"n_rows":48,"n_cols":6,"rows_kept":48,"merged":[[0,0,0,5],[46,0,46,1],[47,0,47,5]],"flags":["formulas_cached_only"]}
["兴企路东侧建筑物拆除明细表"]
["航拍编号","资产名称/用途","建筑面积（㎡）","单价","合价","备注"]
[8,"铁黄干燥工段",1574.35,null,null,"一层高6m、二层高12.2m"]
[9,"铁黄压滤工段",1802.25,null,null,"一层高7.8m、二层高8.3m、302.25㎡为三层其余为两层"]
[10,"精化分厂及空压冷冻站",1030.45,null,null,"1层高6.5m面积451.69㎡、剩余面积二层6.35m、4.3m"]
[11,"铁红压滤工段",1509.91,null,null,"一层高7.9m、二层高8.8m"]
[12,"铁红车间",1574.35,null,null,"一层高5.6m、二层高11.4m"]
[13,"铁红车间办公楼",69.16]
[14,"水井房2",{"v":22.7,"d":"22.70"}]
[15,"传送带通道1",{"v":37.4,"d":"37.40"}]
[16,"氰化分厂办公室",259.88]
[17,"传送带通道2",{"v":30.3,"d":"30.30"}]
[18,"浮选车间",1365.18,null,null,"一层高度5.8m、二层高度8.6m"]
[19,"老氰化分厂 ",561.99,null,null,"证载，层高见勘查表"]
[20,"原料仓",19.08,null,null,"砖混房19.08㎡ 简易房5.94㎡"]
[21,"石灰乳制焙",{"v":233.5,"d":"233.50"},null,null,"高度9.8m 该房产所属珠宝公司"]
[22,"尾渣泵房",{"v":216,"d":"216.00"},null,null,"证载，一层6.2m面积232.54、二层简易房232.54㎡"]
[23,"铁皮房",35.15]
[24,"精艺分厂1",26.91]
[25,"精炼分厂",2885.24,null,null,"层高见勘查表"]
[26,"精艺分厂2",1976.25]
[27,"老贵金属车间",1269.06,null,null,"证载，高度4.1m、4.9m"]
[28,"精炼分厂氯酸钠库房",39.84,null,null,"高度5m"]
[29,"研究中心1",687.28]
[30,"老综合车间1",1447.82,null,null,"868.8㎡层高16.8m、355.02㎡层高4.5m、224㎡层高7.8m、9m"]
[31,"老综合车间2",1124.77,null,null,"746.01㎡高度10m、剩余面积两层4.6m、5.4m"]
[32,"硫铵包装",256.46,null,null,"68.37㎡高度14.7彩板顶；彩板房38.06㎡高度10.15m剩余为砖混一层"]
[33,"碳酸氢铵车间",987.11,null,null,"651.51㎡层高5m、7.63m"]
[34,"综合车间值班室",9.03,null,null,"简易房"]
[35,"研发中心2",75.95]
[36,"压滤机厂房",705.87,null,null,"高度4.9m、3.4m、7.7m"]
[37,"胶带过滤机",579.96,null,null,"高度6.2m 钢构"]
[38,"氰化分厂浸洗工段",{"v":282.1,"d":"282.10"}]
[39,"氰化钠库",621.88,null,null,"包含房顶158.12㎡的彩板房"]
[40,"氰化分厂电解铜车间",6441.12,null,null,"1185.36㎡层高14.9m剩余面积为两层高度为6.3m、8.6m"]
[41,"项目建设指挥部",681.01]
["棚 (4)","铁黄车间外棚",78.88,null,null,"高度6m"]
["棚 (5)","白灰棚",{"v":662.2,"d":"662.20"},null,null,"钢架棚"]
["棚 (6)","东料厂",374.88,null,null,"高度11.1m"]
["棚 (7)","白渣棚",{"v":437.5,"d":"437.50"}]
["棚 (8)","精炼分厂搭棚1",{"v":103.2,"d":"103.20"}]
["棚 (9)","精炼分厂车棚",25.48]
["棚 (10)","精炼分厂变压器盖棚",43.16]
["棚 (11)","精炼分厂氯酸钠库房设备搭棚",{"v":56.4,"d":"56.40"}]
["棚 (12)","精炼分厂搭棚2",125.44]
["棚 (13)","氰化分厂设备搭棚",132.24]
["合计"]
["建筑物拆除要求：地上建筑物全部拆除，地下的独立基础和桩承台全部拆除，装车和外运"]

{"sheet":"构筑物、附属物","index":2,"n_rows":62,"n_cols":8,"rows_kept":62,"merged":[[0,1,0,7],[2,1,2,4],[14,1,14,4],[40,1,40,4],[61,0,61,2]],"flags":["formulas_cached_only"]}
[null,"兴企路东侧构筑物拆除明细表"]
["序号","类别","规格","单位","数量","单价","合价","备注"]
[1,"铁黄、晶种制备、铁红基础区域：（东墙-精炼路）"]
[2,"铁黄生产槽基础","φ7.1m，地下1.5m，地上0.8m，","个",20,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，花岗岩防腐砖，地下有灌注桩"]
[3,"铁黄生产槽基础外硬化",null,"㎡",1798.46,null,null,"地坪贴3层0.4玻璃丝布防腐处理，花岗岩防腐砖"]
[4,"铁黄区滤液槽","深5.0m","㎡",491.18,null,null,"内表面贴8层0.4玻璃丝布防腐处理"]
[5,"罗茨鼓风机基础","地下1.5m，地上0.6m","个",5,null,null,"空压机房北侧"]
[6,"晶种制备基础","φ3.6m，地下1.5m，地上0.8m，","个",24,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，花岗岩防腐砖，地下有灌注桩"]
[7,"晶种制备滤液槽","深5.0m，","㎡",268,null,null,"内表面贴8层0.4玻璃丝布防腐处理"]
[8,"晶种制备基础外硬化",null,"㎡",772.43,null,null,"地坪贴6层0.4玻璃丝布防腐处理，花岗岩防腐砖"]
[9,"铁红区域基础","φ7.1m，地下1.5m，地上0.8m，","个",16,null,null,"基础外表面贴6层0.4玻璃丝布防腐处理，花岗岩防腐砖，地下有灌注桩"]
[10,"铁红区域基础硬化",null,"㎡",1591.85,null,null,"地坪贴3层0.4玻璃丝布防腐处理，花岗岩防腐砖"]
[11,"铁红区滤液槽","深5.0m","㎡",491.18,null,null,"内表面贴6层0.4玻璃丝布防腐处理"]
[12,"氨水罐区（含基础池子）","φ12.5，深2.0m，","个",2,null,null,"含基础"]
[13,"电化学、戈尔反应、直氰氰化基础区域：（南墙-奋进路）"]
[14,"电化学反应池","长14.3m，宽7.3m，深3.3m","㎡",104.39]
[15,"电化学反应槽基础","φ3.0m，地下1.5m，地上0.7m，","个",4]
[16,"电化学反应槽外硬化",null,"㎡",551.54]
[17,"戈尔中水回用槽","长8.4m，宽9.6m，深3.8m","㎡",80.64]
[18,"戈尔反应槽基础","φ3.0m，地下1.5m，地上0.7m","个",3]
[19,"戈尔反应槽基础","φ3.5m，地下1.5m，地上0.5m","个",3]
[20,"戈尔反应槽基础","φ4.0m，地下1.5m，地上0.3m","个",2]
[21,"白灰洞浆槽基础","φ3.5m，地下1.5m，地上0.5m","个",2]
[22,"戈尔微铜沉降槽框架","高4.4m","㎡",74.16]
[23,"基础外硬化",null,"㎡",855.84]
[24,"直氰沉降槽框架","高5.0","㎡",30.18]
[25,"水处理真空泵循环槽","深2.7m","㎡",17.39]
[26,"直氰浓密机","φ6.2m，高6.9m","个",1]
[27,"50围墙","高3.7m","㎡",357.42]
[28,"直氰氰化槽基础","φ4.5m，地下1.5m，地上0.7m","个",8]
[29,"M12浓密机基础","φ14m，高3.0m，","个",3]
[30,"M12浓密机基础","φ14m，高6.2m，","个",2]
[31,"水池","高3.4m","㎡",113.04]
[32,"直氰前液贫液池","高4.3m","㎡",207]
[33,"浓密机滤液池","高4.5m","㎡",81.22]
[34,"浓密机基础","φ6.6m，高3m","个",2]
[35,"浓密机基础上水池","高3.3m","㎡",34.19]
[36,"直氰搅拌槽基础","φ4.2m，地下1.5m，地上0.3m","个",1]
[37,"氰化分厂污水收集池","深2.0m","㎡",40.95]
[38,"24围墙","高3.0m","㎡",1105.8]
[39,"硫铵前液槽、直氰前液贵液贫液槽基础区域：（发展路-和谐路）"]
[40,"24围墙",null,"㎡",54.54,null,null,"研发北围墙"]
[41,"硫铵前液槽基础","φ4.0m，地下1.5m，地上0.1m","个",3,null,null,"基础外表面贴3层0.4玻璃丝布防腐处理，防腐瓷板，"]
[42,"M15浓密机池","φ17m，高3m，地下φ8m，深3.2m壁厚0.5","个",1,null,null,"浓密机内表面贴10层0.4玻璃丝布防腐处理，防腐标砖"]
[43,"M18浓密机池","φ21m，高5.1m，地下φ8m，深3.2m，2个","个",2,null,null,"浓密机内表面贴10层0.4玻璃丝布防腐处理，防腐标砖"]
[44,"M25浓密机池","φ28m，高5.1m，地下φ8m，深3.2m","个",2,null,null,"浓密机内表面贴10层0.4玻璃丝布防腐处理，防腐标砖"]
[45,"前液贵液贫液槽","深4.0m","㎡",499.8,null,null,"内表面贴贴10层0.4玻璃丝布防腐处理"]
[46,"氰化槽基础","φ5.5m，地上1.5m，地下1.5m","个",15]
[47,"高效浓密机基础","φ10.5m，高8.6m，","个",2]
[48,"电解雨水收集池","深5.0m","㎡",85.49]
[49,"兴企路东侧水泥地坪"]
[50,"水泥地坪4",null,"㎡",6151.15]
[51,"水泥地坪5",null,"㎡",1156]
[52,"水泥地坪12",null,"㎡",181.63]
[53,"水泥地坪13",null,"㎡",407.18]
[54,"水泥地坪14",null,"㎡",234]
[55,"水泥地坪15",null,"㎡",338.99]
[56,"水泥地坪16",null,"㎡",476]
[57,"水泥地坪19",null,"㎡",427.24]
[58,"水泥地坪23",null,"㎡",5291.92]
[59,"水泥路面，园区道路","含路边排水沟和基础","㎡",5012.79]
["合计"]